ON/OFF Switch – switches ON/OFF the device

LCD Display – displays real-time values of LiDAR and accelerometer sensors

LiDAR sensor module – obtains bank full-width of freshwater body

Laser – assist in accuracy of data collection

Scope – assist in accuracy of data collection